# Time when the point is captured
float32 time

# Converted distance in the sensor frame
float64 x
float64 y
float64 z

# Raw measurement from Leishen C16
float64 azimuth
float64 distance
float64 intensity
